Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Mark the Rackmounting Location

Use the rackmounting template to identify the correct mounting holes for the shelf rails.

Note - Load the rack from bottom to top.

1. Ensure that there is enough vertical space in the cabinet to install the server.
2. Place the rackmounting template against the front rails.

   The bottom edge of the template corresponds to the bottom edge of the server. Measure up from the bottom of the template.

3. Mark the mounting holes for the front shelf rails.
4. Mark the mounting holes for the rear shelf rails.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |