Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Remove the Service Processor Card

The service processor card is a cold-service component that can be replaced by a customer.

1. Back up the SP configuration information before removing the service processor card.

   At the Oracle ILOM prompt, type:

       -> cd /SP/config
       -> dump -destination uri target

   where:

   - The acceptable values for uri are:
     - tftp
     - ftp
     - sftp
     - scp
     - http
     - https
   - target is the remote location where you will want to store the configuration information.

   For example:

       -> dump -destination tftp://129.99.99.99/pathname

2. Remove the main module from the server.

   See Remove the Main Module.

3. Take the necessary ESD precautions.

   See Prevent ESD Damage.

4. Locate the service processor card on the main module.

   See Main Module Components.

5. Grasp the service processor card by the two grasp points, and lift up to disengage the service processor card from the connectors on the motherboard.
6. Lift the service processor card up and away from the motherboard.

##### Related Information

- Service Processor Card Overview

- Locate a Faulty Service Processor Card

- Install the Service Processor Card

- Verify Service Processor Card Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |