Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Check for Faults (`show` `faulty` Command)

Use the `show` `faulty` command to display information about faults and alerts diagnosed by the system.

See Fault Management Command Examples for examples of the kind of information the command displays for different types of faults.

- At the `->` prompt, enter the `show` `faulty` command.

      -> show faulty
      Target              | Property               | Value
      --------------------+------------------------+-------------------------------
      /SP/faultmgmt/0     | fru                    | /SYS/PS0
      /SP/faultmgmt/0/    | class                  | fault.chassis.power.volt-fail
      faults/0            |                        |
      /SP/faultmgmt/0/    | sunw-msg-id            | SPT-8000-LC
      faults/0            |                        |
      /SP/faultmgmt/0/    | uuid               | 59654226-50d3-cdc6-9f09-e591f39792ca
      faults/0            |                        |
      /SP/faultmgmt/0/    | timestamp              | 2010-08-11/14:54:23
      faults/0            |                        |
      /SP/faultmgmt/0/    | fru_part_number        | 3002235
      faults/0            |                        |
      /SP/faultmgmt/0/    | fru_serial_number      | 003136
      faults/0            |                        |
      /SP/faultmgmt/0/    | product_serial_number  | BDL1024FDA
      faults/0            |                        |
      /SP/faultmgmt/0/    | chassis_serial_number  | BDL1024FDA
      faults/0            |                        |
      /SP/faultmgmt/0/    | detector               | /SYS/PS0/VOLT_FAULT
      faults/0            |                        |

##### Related Information

- Diagnostics Process

- Clear Faults (`clear_fault_action` Property)

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |