Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Server Overview

The SPARC T4-4 is a 5-rack unit (5U) server.

Figure 1 SPARC T4-4 Server

Component/Function | New Characteristics
--- | ---
Processor | Up to 4x SPARC T4, 16-core chip multiprocessor (CMP) with 8 threads per core. 2x multiprocessor configuration also available.
Memory | 16x DDR3 DIMM slots; 4 Gbyte, 8 Gbyte, and 16 GByte capacity modules.
I/O - Expansion | 16x PCIe Gen2 card slots. 4x Gigabit Ethernet ports. 4x external USB ports. Optional 8x 10-Gigabit Ethernet ports.
Hard drive storage | 8-disk capable backplane. Any mix of hard drives and solid state drives supported
Service processor | Modular, pluggable on the motherboard.

##### Related Information

- Confirming Specifications

- Shipping Kit

- Handling Precautions

- Tools Needed for Installation

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |