Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the System Battery

1. Insert the new system battery in the main module, with the positive side (+) facing out.
2. Install the main module back into the server.

   See Install the Main Module.

3. If the service processor is configured to synchronize with a network time server using the Network Time Protocol (NTP), the ILOM clock will be reset as soon as the server is powered on and connected to the network. Otherwise, proceed to the next step.
4. If the service processor is not configured to use NTP, you must reset the ILOM clock using the ILOM CLI or the web interface. For instructions, see the Oracle Integrated Lights Out Manager (ILOM) 3.0 Documentation Collection.
5. If the service processor is not configured to use NTP, use the ILOM `clock` command to set the day and time.

   The following example sets the date to June 17, 2010, and the time zone to GMT.

       -> set /SP/clock datetime=061716192010

       -> show /SP/clock

       /SP/clock
           Targets:

           Properties:
               datetime = Wed JUN 17 16:19:56 2010
               timezone = GMT (GMT)
               usentpserver = disabled
           Commands:
               cd
               set
               show

   Note - For additional details about setting the ILOM clock, refer to the CLI Procedures Guide for Oracle ILOM.

6. Verify that the new system battery is functioning properly.

   See Verify the System Battery.

##### Related Information

- Remove the System Battery

- Verify the System Battery

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |