Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Processor Module LEDs

No. | LED | Icon | Description
--- | --- | --- | ---
1 | Ready to Remove (blue) |  | (Not supported.)
2 | Service Required (amber) |  | Indicates that the processor module has experienced a fault condition.
3 | OK (green) |  | Indicates if the processor module is available for use. On – The server is running and the processor module is powered up. Off – The server is powered down and the processor module is in standby mode. If the server is powered on, then this indicates that the processor module is powered down (the blue Ready to Remove LED will be lit in this case).

##### Related Information

- Processor Module Overview

- Locate a Faulty Processor Module

- Remove a Processor Module

- Install a Processor Module

- Verify Processor Module Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |