Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Configure POST

1. Access the Oracle ILOM `->` prompt.

   See Access the SP (Oracle ILOM).

2. Set the virtual keyswitch to the value that corresponds to the POST configuration you want to run.

   The following example sets the virtual keyswitch to normal, which will configure POST to run according to other parameter values.

       -> set /SYS keyswitch_state=normal
       Set ‘keyswitch_state' to ‘Normal'

   For possible values for the `keyswitch_state` parameter, see Oracle ILOM Properties That Affect POST Behavior.

3. If the virtual keyswitch is set to `normal`, and you want to define the `mode`, `level`, `verbosity`, or `trigger`, set the respective parameters.

   Syntax:

   `set /HOST/diag` property`=`value

   See Oracle ILOM Properties That Affect POST Behavior for a list of parameters and values.

   Examples:

       -> set /HOST/diag mode=normal
       -> set /HOST/diag verbosity=max

4. To see the current values for settings, use the `show` command.

   Example:

       -> show /HOST/diag

       /HOST/diag
           Targets:

           Properties:
               level = min
               mode = normal
               trigger = power-on-reset error-reset
               verbosity = normal

           Commands:
               cd
               set
               show
       ->

##### Related Information

- POST Overview

- Oracle ILOM Properties That Affect POST Behavior

- Run POST With Maximum Testing

- Interpret POST Fault Messages

- Clear POST-Detected Faults

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |