Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Clear Faults (`clear_fault_action` Property)

Use the `clear_fault_action` property of a FRU with the `set` command to manually clear Oracle ILOM-detected faults from the SP.

If Oracle ILOM detects the FRU replacement, it will automatically clear the fault so that manual clearing of the fault is not necessary. For PSH diagnosed faults, if the replacement of the FRU is detected by the system or the fault is manually cleared on the host, the fault will also be cleared from the SP. In such cases, manual fault clearing will typically not be required.

Note - For PSH-detected faults, this procedure clears the fault from the SP but not from the host. If the fault persists in the host, clear it manually as described in Clear PSH-Detected Faults.

- At the `->` prompt, use the `set` command with the `clear_fault_action=True` property.

  This example begins with an excerpt from the `fmadm` `faulty` command showing power supply 0 with a voltage failure. After the fault condition is corrected (a new power supply has been installed), the fault state is cleared manually.

  Note - In this example, the characters “SPT” at the beginning of the message ID indicate that the fault was detected by Oracle ILOM.

      [...]

      faultmgmtsp> fmadm faulty
      ------------------- ------------------------------------ -------------- -------
      Time                UUID                                 msgid          Severity
      ------------------- ------------------------------------ -------------- -------
      2010-08-27/19:46:26 edc898a3-c875-6b86-851a-91a4ed8ad58e SPT-8000-MJ    Critical
      Fault class : fault.chassis.power.fail

      FRU         : /SYS/PS0
                       (Part Number: 300-2159-05)
                       (Serial Number: 1908BAO-1020A90156)

      Description : A Power Supply has failed and is not providing power to the
                       server.
      [...]

      -> set /SYS/PS0 clear_fault_action=true
      Are you sure you want to clear /SYS/PS0 (y/n)? y

      -> show

       /SYS/PS0
          Targets:
              VINOK
              PWROK
              CUR_FAULT
              VOLT_FAULT
              FAN_FAULT
              TEMP_FAULT
              V_IN
              I_IN
              V_OUT
              I_OUT
              INPUT_POWER
              OUTPUT_POWER
          Properties:
              type = Power Supply
              ipmi_name = PS0
              fru_name = /SYS/PS0
              fru_description = Powersupply
              fru_manufacturer = Delta Electronics
              fru_version = 03
              fru_part_number = 3002235
              fru_serial_number = 003136
              fault_state = OK
              clear_fault_action = (none)

          Commands:
              cd
              set
              show

##### Related Information

- Diagnostics Process

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |