Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Remove the Main Module

1. Shut down the server.

   See Removing Power From the Server.

2. Locate the main module in the server.

   See Front Panel Components.

3. Squeeze the release latches together on the two extraction levers and pull the extraction levers out to disengage the main module from the server.
4. Pull the main module halfway out of the server.
5. Press the levers back together, toward the center of the main module.

   This will keep the levers from getting damaged when you remove the main module from the server.

6. Remove the cover from the main module:
   1. Press down on the green button at the top of the cover to disengage the cover from the main module.
   2. Keeping the button pressed down, push the cover toward the rear of the main module and lift the cover up and away from the main module.
7. Service the component inside the main module.

   The following components are accessible inside the main module:

   - Servicing RAID Expansion Modules

   - Servicing the Service Processor Card

   - Servicing the System Battery

   - Servicing the System Configuration PROM

   - Servicing the Front I/O Assembly

   - Servicing the Storage Backplane

##### Related Information

- Install the Main Module

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |