Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Verify Service Processor Card Functionality

1. Verify that the SP Status LED on the main module or rear I/O module is lit green.

   See Main Module Motherboard LEDs or Rear I/O Module LEDs.

2. Verify that the front and rear Service Required LEDs are not lit.

   See Interpreting Diagnostic LEDs.

3. Perform one of the following tasks based on your verification results:

   - If the previous steps did not clear the fault, see Diagnostics Process.

   - If the previous steps indicate that no faults have been detected, then the service processor card has been replaced successfully. No further action is required.

##### Related Information

- Service Processor Card Overview

- Locate a Faulty Service Processor Card

- Remove the Service Processor Card

- Install the Service Processor Card

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |