Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

### Powering On the Server for the First Time

These topics include instructions for booting the server and for enabling the service processor network management port.

Step | Description | Links
--- | --- | ---
1 | Connect a serial terminal device or terminal server to the SER MGT port. | Connect a Terminal or Emulator to the SER MGT Port
2 | Prepare the power cords. | Prepare Power Cords
3 | Power on the server for the first time. | Power On the System for the First Time
4 | Set Oracle Solaris OS configuration parameters. | Oracle Solaris OS Configuration Parameters
5 (Optional) | Configure the NET MGT port to use a static IP address. | Assigning a Static IP Address to the SP
6 | Boot the Oracle Solaris OS. | Booting the Oracle Solaris Operating System

##### Related Information

- Confirming Server and Site Specifications

- Connecting the Server Cables

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |