Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the Rear Shipping Bracket

1. Remove the bottom two rear rackmount screws on each side (four total).

   The server is held in place by the four top screws (two on each side).

2. Hold the lower shipping bracket in place
3. Install two No. 2 Phillips screws in the bottom holes of the lower shipping bracket.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |