Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### FRU Reference

The following table identifies the server components that are field-replaceable.

Table 15 List of Field-Replaceable Units

Description | Quantity | FRU Name | Remove and Replace Instructions
--- | --- | --- | ---
Processor module | 1 or 2 | `/SYS/PMn` | Servicing Processor Modules
DIMM | 16 or 32 | `/SYS/PMn/CMP` n`/BOB` n`/CH` n`/D` n | Servicing DIMMs
Hard drive | 1 to 8 | `/SYS/MB/HDD` n | Servicing Hard Drives
Power supply | 4 | `/SYS/PS` n | Servicing Power Supplies
RAID expansion module | 2 | `/SYS/MB/REM` n | Servicing RAID Expansion Modules
Service processor card | 1 | `/SYS/MB/SP` | Servicing the Service Processor Card
System battery | 1 | `/SYS/MB/BAT` | Servicing the System Battery
Fan module | 5 | `/SYS/FM` n | Servicing Fan Modules
Express module | 0 to 16 | `/SYS/PCI-EMn` | Servicing Express Modules
Rear I/O module | 1 | `/SYS/RIO` | Servicing the Rear I/O Module
System configuration PROM | 1 | `/SYS/MB/SCC` | Servicing the System Configuration PROM
Front I/O assembly | 1 | `/SYS/MB/FIO` | Servicing the Front I/O Assembly
Storage backplane | 2 | `/SYS/MB/SASBP` n | Servicing the Storage Backplane
Main module motherboard | 1 | `/SYS/MB` | Servicing the Main Module Motherboard
Rear chassis subassembly | 1 | N/A | Servicing the Rear Chassis Subassembly

##### Related Information

- Removing Power From the Server

- Returning the Server to Operation

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |