Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the Main Module

1. Place the cover back onto the main module and slide the cover forward until the latch clicks into place.
2. Insert the main module back into its slot in the server.
3. Press the levers back together, toward the center of the module, and press them firmly against the module to fully seat the module back into the server.

   The levers should click into place when the module is fully seated in the server.

4. Power on the server.

   See Returning the Server to Operation.

##### Related Information

- Remove the Main Module

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |