Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Cold Service, Replacement by Authorized Service Personnel

The following components must be replaced by authorized service personnel. These replacement procedures can only be done when the server is powered down and power cables are unplugged.

Authorized Service Personnel Only - Cold Service (power down server and disconnect power cables) | Notes
--- | ---
System configuration PROM |
Front I/O assembly |
Storage backplane |
Main module motherboard | Transfer system configuration PROM to new motherboard
Rear chassis subassembly |

See Power Off the Server (SP Command) for the procedure to shut down the server.

##### Related Information

- Removing Power From the Server

- Accessing Internal Components

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |