Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### DIMM FRU Names

DIMM FRU IDs are based on the location of the DIMM slot on the processor module, as well as in which slot the processor module is installed. For example, the full FRU ID for the leftmost DIMM slot (`BOB1/CH0/D0`) on a processor module installed at PM0 is:

`/SYS/PM0/CMP1/BOB1/CH0/D0`

Table 21 DIMM FRU Names

Associated CMP | DIMM FRU Name (From Left to Right on Processor Module) | Slot Color
--- | --- | ---
`/SYS/PMx/CMP1` | `/SYS/PMx/CMP1/BOB1/CH0/D0` `/SYS/PMx/CMP1/BOB1/CH0/D1` `/SYS/PMx/CMP1/BOB1/CH1/D0` `/SYS/PMx/CMP1/BOB1/CH1/D1` `/SYS/PMx/CMP1/BOB0/CH1/D1` `/SYS/PMx/CMP1/BOB0/CH1/D0` `/SYS/PMx/CMP1/BOB0/CH0/D1` `/SYS/PMx/CMP1/BOB0/CH0/D0` `/SYS/PMx/CMP1/BOB3/CH0/D0` `/SYS/PMx/CMP1/BOB3/CH0/D1` `/SYS/PMx/CMP1/BOB3/CH1/D0` `/SYS/PMx/CMP1/BOB3/CH1/D1` `/SYS/PMx/CMP1/BOB2/CH1/D1` `/SYS/PMx/CMP1/BOB2/CH1/D0` `/SYS/PMx/CMP1/BOB2/CH0/D1` `/SYS/PMx/CMP1/BOB2/CH0/D0` | White Black Blue Black Black Blue Black White White Black Blue Black Black Blue Black White
`/SYS/PMx/CMP0` | `/SYS/PMx/CMP0/BOB1/CH0/D0` `/SYS/PMx/CMP0/BOB1/CH0/D1` `/SYS/PMx/CMP0/BOB1/CH1/D0` `/SYS/PMx/CMP0/BOB1/CH1/D1` `/SYS/PMx/CMP0/BOB0/CH1/D1` `/SYS/PMx/CMP0/BOB0/CH1/D0` `/SYS/PMx/CMP0/BOB0/CH0/D1` `/SYS/PMx/CMP0/BOB0/CH0/D0` `/SYS/PMx/CMP0/BOB3/CH0/D0` `/SYS/PMx/CMP0/BOB3/CH0/D1` `/SYS/PMx/CMP0/BOB3/CH1/D0` `/SYS/PMx/CMP0/BOB3/CH1/D1` `/SYS/PMx/CMP0/BOB2/CH1/D1` `/SYS/PMx/CMP0/BOB2/CH1/D0` `/SYS/PMx/CMP0/BOB2/CH0/D1` `/SYS/PMx/CMP0/BOB2/CH0/D0` | White Black Blue Black Black Blue Black White White Black Blue Black Black Blue Black White

##### Related Information

- DIMM Population Rules (Except 1536-Gbyte Configurations)

- Understanding the Supported Memory Configurations

- DIMM Rank Classification

- Understanding DIMM Configuration Error Messages

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |