Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Display FRU Information (`show` Command)

Use the Oracle ILOM `show` command to display information about individual FRUs.

- At the `->` prompt, type the `show` command.

  In the following example, the `show` command displays information about a DIMM.

      -> show /SYS/PM0/CMP0/BOB0/CH0/D0

      /SYS/PM0/CMP0/BOB0/CH0/D0
         Targets:
             PRSNT
             T_AMB
             SERVICE

         Properties:
             Type = DIMM
             ipmi_name = BOB0/CH0/D0
             component_state = Enabled
             fru_name = 2048MB DDR3 SDRAM
             fru_description = DDR3 DIMM 2048 Mbytes
             fru_manufacturer = Samsung
             fru_version = 0
             fru_part_number = M393B5673FH0-CH9
             fru_serial_number = 80CE01100506036C9D
             fault_state = OK
             clear_fault_action = (none)

      Commands:
      cd
      set
      show

##### Related Information

- Diagnostics Process

- Clear Faults (`clear_fault_action` Property)

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |