Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Acoustic Noise Emissions

Declared noise emissions for the SPARC T4-4 server is in accordance with ISO 9296 standards.

Description | Operating at Idle | Operating at Maximum Power
--- | --- | ---
Sound power level, LwAd (1 B = 10 dB) | 7.4 B | 8.2 B
Sound Pressure Level, LpAm (bystander positions) | 63 dBA | 68.2 dBA

##### Related Information

- Input Power Information

- Environmental Requirements

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |