Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Power On the System for the First Time

Before You Begin

Complete the following tasks:

- Confirm that you have completed the installation of the server in its rack. See Installing the Server.

- Attach the cable management assembly. See Install the CMA.

- Connect a terminal or terminal emulator to the SER MGT port. See Connect a Terminal or Emulator to the SER MGT Port.

1. (Optional) Connect an Ethernet cable between the server's NET MGT port and the network to which future connections to the SP and host will be made. See Connect the NET MGT Cable.

   After the initial configuration of the server using the SER MGT port, communication with the SP and host is usually performed through this Ethernet interface.

2. Connect an Ethernet cable between one of the server's NET ports (Rear Panel Components) and the network to which the server will communicate.
3. Plug the power cords into the power supplies and into a power source.

   Note - Only two power connections are required for operation. Use four power connections and two separate circuits for redundancy.

   The service processor runs on the 3.3V standby voltage. As soon as AC power is connected to the server, the service processor powers on, runs diagnostics, and initializes the ILOM firmware.

   After a few minutes, the SP login prompt appears on the terminal device. The host is not initialized or powered on yet.

4. At the terminal device, log in to the SP as `root` with a password of `changeme`.

       XXXXXXXXXXXXXXXX login: root
       Password: changeme
       . . .
       ->

   After a brief delay, the Oracle ILOM prompt is displayed (`->`).

   Note - To enable first-time login and access to Oracle ILOM, a default Administrator account and its password are provided with the system. To build a secure environment, you must change the default password (`changeme`) for the default Administrator account (`root`) after your initial login to Oracle ILOM. If this default Administrator account has been changed, contact your system administrator for an Oracle ILOM user account with Administrator privileges.

   For more information about the administration tasks such as changing passwords, adding accounts, and setting account privileges, refer to the Oracle ILOM documentation.

   Note - By default, the SP is configured to use DHCP to obtain an IP address. If you plan to assign a static IP address to the SP, seeAssign a Static IP Address to the NET MGT Port for more instructions.

5. Open a second terminal device and log in to the SP as `root`.

   After a brief delay, the SP prompt is displayed (`->`). At this point, there are many commands you can perform using the ILOM interface.

6. In the first terminal device, redirect the host output to display on the serial terminal device:

       -> start /SP/console
       Are you sure you want to start /SP/console (y/n)? y
       Serial console started. To stop, type #.
       . . .

   After you start the SP console, the server initialization takes approximately 20 minutes to complete. This terminal device displays all SP console messages during intial boot.

7. In the second terminal device, power on the server:

       -> start /SYS
       Are you sure you want to start /SYS (y/n)? y

   This terminal device displays all system console messages during initial boot.

8. When prompted, follow the onscreen instructions for configuring the Oracle Solaris Operating System on your host and enter the following configuration information.

   You will be prompted to confirm the configuration several times, enabling confirmation and changes. If you are not sure how to respond to a particular value, you can accept the default, and make future changes when the Oracle Solaris OS is running. See Oracle Solaris OS Configuration Parameters for a description of the Oracle Solaris OS parameters you must provide during initial configuration.

9. Log in to the server and explore its capabilities.

   There are many commands you can use to verify the functionality of the server. The following list describes a few of them:

   - `showrev` – Displays the host name and server architecture information. Use the `-a` option with this command to see the patches that are installed.
   - `psrinfo` – Displays information about the number and status of the processors and cores in the host.
   - `prtdiag` – Displays server configuration and diagnostic information.

   Review the Oracle Solaris OS man pages and documentation for more details.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |