4.6. Graphics
Prev | Chapter 4. Sun Ray 3i Client | Next

## 4.6. Graphics

The Sun Ray 3i Client features a high-performance integrated graphics engine embedded in the CPU to provide high-resolution graphics to the LCD panel, as well as one analog external monitor or projector that can support 1920x1080 @ 60Hz as an input resolution. The output resolution is always locked to the resolution of the internal display (1920x1080 @ 60Hz), and the internal display resolution cannot be changed.

Note

Use of an analog external device requires a DVI-I to HD-15 adapter (not supplied with the unit).

Prev | Up | Next
4.5. Flat Panel Display | Home | 4.7. Network Interfaces