2.7. Power Supply
Prev | Chapter 2. Sun Ray 3 Client | Next

## 2.7. Power Supply

The power supply unit (PSU) is a 36W AC/DC external power adapter that meets the specifications for external power adapters as listed in the EPA document, ENERGY STAR Program Requirements for Computers Version 5.0. Power supply inputs and outputs are listed in the following table.

Table 2.3. Sun Ray 3 Client PSU Inputs and Outputs

AC Input socket | IEC 60320 Type C8 (matches C7 plug)
DC Output | 12 Volts DC at 3.0 Amps

Prev | Up | Next
2.6. Network Interfaces | Home | 2.8. MTBF, Reliability, and Other Standards