5.3. Energy Efficiency
Prev | Chapter 5. Environmental Data | Next

## 5.3. Energy Efficiency

All Sun Ray 3 Series Clients are highly energy efficient, using power management features designed to meet the specifications for Thin Clients in ENERGY STAR Program Requirements for Computers Version 5.0, published by the U.S. Department of Energy.

The following tables list the power requirements for Sun Ray 3 Series Clients.

Table 5.1. Sun Ray 3 Client Operational Mode Power Requirements

Mode | ENERGY STAR Requirement (Category A) | Typical Usage for Sun Ray 3 Client
--- | --- | ---
Off Mode | ≤ 2 W | 0.5 W
Idle State | ≤ 12 W | 6 W

Table 5.2. Sun Ray 3 Plus Client Operational Mode Power Requirements

Mode | ENERGY STAR Requirement (Category B) | Typical Usage for Sun Ray 3 Plus Client
--- | --- | ---
Off Mode | ≤ 2 W | 0.31 W
Idle State | ≤ 15 W | 14.2 W

Table 5.3. Sun Ray 3i Client Operational Mode Power Requirements

Mode | ENERGY STAR Requirement (Category A) | Typical Usage for Sun Ray 3i Client
--- | --- | ---
Off Mode | ≤ 2 W | 0.39 W
Idle State | ≤ 12 W | 5.38 W

Prev | Up | Next
5.2. Restrictions on Materials and Substances | Home | 5.4. Recyclability