5.4. Recyclability
Prev | Chapter 5. Environmental Data | Next

## 5.4. Recyclability

The material choices and design of the Sun Ray 3 Series Clients maximize ease of disassembly, safe recycling, and transportation efficiency. Assessment results are summarized in the following tables. Weights listed exclude the keyboard and mouse.

Note

Sun Ray 3 Series Clients contain 0% recycled materials (by weight).

Table 5.4. Sun Ray 3 Client Recyclability

Product Recyclability Assessment | Category sub-total Weights (g) | Actual (%) | WEEE Recyclability Requirements (%)
--- | --- | --- | ---
Recyclable | 765 | 92% | ≥ 65%
Waste to Energy | 50 | 6% | ≤ 10%
Landfill | 13 | 2% | ≤ 25%
Total Weight | 828 | 100% | --

Table 5.5. Sun Ray 3 Plus Client Recyclability

Product Recyclability Assessment | Category sub-total Weights (g) | Actual (%) | WEEE Recyclability Requirements (%)
--- | --- | --- | ---
Recyclable | 1,086 | 90% | ≥ 65%
Waste to Energy | 105 | 9% | ≤ 10%
Landfill | 15 | 1% | ≤ 25%
Total Weight | 1,206 | 100% | --

Table 5.6. Sun Ray 3i Client Recyclability

Product Recyclability Assessment | Category sub-total Weights (g) | Actual (%) | WEEE Recyclability Requirements (%)
--- | --- | --- | ---
Recyclable | 5,518 | 98% | ≥ 65%
Waste to Energy | 59 | 1% | ≤ 10%
Landfill | 40 | 1% | ≤ 25%
Total Weight | 5,617 | 100% | --

Note

The internal fluorescent lamps in Sun Ray 3i Client displays contain mercury. Handle the display and the complete unit with care and dispose according to state or local laws.

Prev | Up | Next
5.3. Energy Efficiency | Home | 5.5. Packaging