3.7. Power Supply
Prev | Chapter 3. Sun Ray 3 Plus Client | Next

## 3.7. Power Supply

The power supply unit (PSU) is a 36W AC/DC external power adapter that meets the specifications for external power adapters as listed in the EPA document, ENERGY STAR Program Requirements for Computers Version 5.0. Power supply inputs and outputs are listed in the following table.

Table 3.4. Sun Ray 3 Plus Client PSU Inputs and Outputs

AC Input | 90-264V, 47-63 Hz
AC Input socket | IEC320 Type C7 (matches C8 plug)
DC Output | 12 Volts VDC at 3.0 Amps

Prev | Up | Next
3.6. Network Interfaces | Home | 3.8. MTBF, Reliability, and Other Standards