Skip Navigation Links
Exit Print View
| Oracle Solaris Cluster Reference Manual Oracle Solaris Cluster 4.1

Search Scope:

- This Document
- Entire Library

### SUNW.SCTelemetry

### , SCTelemetry

- resource type for collecting data on system resource usage

## Description

`SUNW.SCTelemetry` is the resource type that enables you to collect data on the usage of system resources. `SUNW.SCTelemetry` stores system resource usage data in a Java DB database for seven days. The resource of type `SUNW.SCTelemetry` has a dependency on the resource of type `SUNW.derby`. For more information, see the `SUNW.derby`(5) man page.

The extension properties associated with the `SUNW.SCTelemetry` resource type are as follows:

`Extended_accounting_cleanup`(boolean)

  Specifies whether the extended accounting log file is cleaned up, that is whether historical data is deleted. Possible values for `Extended_accounting_cleanup` are `TRUE` and `FALSE`.

  Category

    Optional

  Default

    TRUE

  Tunable

    Any time

`Monitor_retry_count`(integer)

  Controls fault-monitor restarts. The property indicates the number of times that the process monitor facility restarts the fault monitor. The property corresponds to the `-n` option passed to the `pmfadm`(1M) command. The Resource Group Manager (RGM) counts the number of restarts in a specified time window. See the `Monitor_retry_interval` property for more information. Note that `Monitor_retry_count` refers to the restarts of the fault monitor itself, not to the resource of type `SUNW.SCTelemetry`.

  Category

    Optional

  Default

    4

  Tunable

    Any time

`Monitor_retry_interval`(integer)

  Indicates the time window in minutes during which the RGM counts fault-monitor failures. The property corresponds to the `-t` option passed to the `pmfadm`(1M) command. If the number of times the fault monitor fails exceeds the value of the `Monitor_retry_count` property, the process monitor facility does not restart the fault monitor.

  Category

    Optional

  Default

    2 minutes

  Tunable

    Any time

`Probe_timeout`(integer)

  Specifies the timeout value, in seconds, for the probe.

  Category

    Optional

  Default

    60 seconds

  Minimum

    2 seconds

  Tunable

    Any time

`Sampling_interval`(integer)

  Specifies how often monitoring data is collected. The `Telemetry_sampling_interval` property must have a value of between `30` and `3600`.

  Category

    Mandatory

  Default

    60

  Minimum

    30 seconds

  Maximum

    3600 seconds

  Tunable

    Any time

## See Also

`pmfadm`(1M), `SUNW.derby`(5)

Copyright © 2000, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |