Skip Headers

StorageTek SL150 Modular Tape Library Customer Replaceable Unit Guide 29812-05 |
| Library | Contents | Index

Previous | Next |

# 2 Preparations

This chapter introduces general topics for your consideration before performing a CRU removal or replacement procedure.

## Electrostatic Discharge

Be aware of the precautions needed when handling parts. A discharge of static electricity from a finger or other conductor might damage static-sensitive devices. This type of damage may reduce the life expectancy of the product.

### Electrostatic Discharge Prevention

- Avoid hand contact by transporting and storing products in static-safe containers.

- Keep electrostatic-sensitive parts in their containers until they arrive at static-free work areas.

- Place parts on a grounded surface before removing from their containers.

- Avoid touching pins, leads, or circuitry.

- Use proper grounding practices when touching a static-sensitive component or assembly.

### Grounding Methods to Prevent Electrostatic Discharge

Use one or more of the following methods when handling or installing electrostatic-sensitive parts:

- Use a wrist strap connected by a ground cord to a grounded chassis.

- Use conductive field service tools.

- Use a portable field service kit with a folding static-dissipating work mat.

  Note: If you do not have any of the suggested equipment for proper grounding, arrange for an authorized reseller to install the part.

## SL150 Remote Interface

The process of removing and replacing customer replaceable units (CRUs) relies on functions and commands in the SL150 remote interface (GUI). It is assumed that you are familiar with the library tab of that interface.

You access the remote interface by entering the library hostname or IP address in a supported web browser. The login dialog is shown in Figure 2-1. Note the Help link in the upper right of the screen.

Refer to the user's guide (`http://docs.oracle.com`) or the Help system to gain familiarity before attempting any removal or replacement action.

Figure 2-1 SL150 Remote Management Log In Dialog

Illustration Legend:

1 - User ID

2 - Password

3 - Help Link