Omitir Vínculos de navegación
Salir de la Vista de impresión
| Guía de instalación de Sun Blade X4-2B para software ESX

Rate this document:

Ámbito de búsqueda:

- Este documento
- Toda la biblioteca

Please tell us how to improve our documentation:
Provide more details about the topic on this page
Fix incorrect information
Provide missing information
Provide translated version
Other
Your rating has been updated
Thank you for your feedback!
If you want to participate in content improvement and share additional information, please click
Feedback button.

### Instalación de los controladores de VMware ESXi 5

Si tiene Sun Blade 6000 Virtualized 40GbE NEM instalado en el chasis, debe instalar un controlador para este NEM. Los otros NEM admitidos por Sun Blade X4-2B no requieren controladores adicionales.

Para instalar los controladores para Sun Blade 6000 Virtualized 40GbE NEM, realice lo siguiente:

1. Busque lo siguiente en el sitio de VMware:

   VMware ESXi 5.0 Driver CD for Oracle Sun Blade 6000 Virtualized Network Express Module - 7100090

2. Descargue los controladores.
3. Instale los controladores.
4. Reinicie el servidor.

Pasos siguientes

- Actualización de VMware ESXi 5

Copyright © 2013, Oracle y/o sus filiales. Todos los derechos reservados. Advertencia legal |